**Channel Islands OOG Booking Request**

**OUT OF GAUGE SHIPMENT GUIDANCE**

**Jersey**

When shipping vehicles into Jersey that are considered out of gauge a P30 exemption permit is required, to obtain the permit customers must apply via the Gov.je website. [Vehicles which need exemption permits (P30)](https://www.gov.je/Travel/Motoring/OversizedVehicles/pages/p30.aspx#:~:text=%E2%80%8B%E2%80%8B%E2%80%8B%E2%80%8BWhat%20vehicles%20need%20a%20P30%20permit,-The%20following%20vehicles&text=vehicles%20or%20trailers%20over%202.3,6.7%20metres%20(22%20feet)%20long) Application form [Apply for a temporary exemption permit (P30)](https://www.gov.je/Travel/Motoring/OversizedVehicles/Pages/ExemptionForm.aspx)

For vehicles shipping to Jersey the P30 exemption must be completed and authorised before booking confirmed.

**What vehicles require a P30 permits**

The following vehicles are not allowed on Jersey roads without a permit:

* Vehicles or trailers over 2.3 metres (7 feet and 6.5 inches) wide
* Rigid vehicles over 9.3 metres (30 feet and 6 inches) long
* Articulated vehicles over 11 metres (36 feet and 1 inch) long
* Trailers (draw bar type) over 6.7 metres (22 feet) long
* Vehicles with a maximum axle weight over 10,500 kilograms
* Vehicles with a gross weight over 32,000 kilograms

**Portsmouth**

Vehicles exceeding the listed below dimensions must pre notify the port 72 hours prior to shipment (vehicles should **NOT** arrive for shipment any longer than 12 hours prior to scheduled departure)

OOG notification and PiP OOG load sheet should be completed by the customer submitted via e mail to [jersey.fbookings@dfds.com](mailto:jersey.fbookings@dfds.com)

E mail the Completed OOG notification and PiP OOG load sheet to [freight@portsmouth-port.co.uk](mailto:freight@portsmouth-port.co.uk)

Note to be added in internal remarks **awaiting approval do not ship**, once approved has been granted remarks to be removed,

Out of gauge request are required when the vehicle dimensions exceed the following:

* Weight:Total gross weight : Exceeds **50000kg**
* Single axel weight: Exceeds **12000kg** (This is a specific requirement to Jersey)
* Height: **4.8m**
* Width: **3.0m**
* Length: **18.75m**

Vessel restrictions

**Maximum restrictions are dependent on the berth being used**

|  |  |  |  |
| --- | --- | --- | --- |
| **Berth** | **Max Tonnage** | **Max Width** | **Max Height** |
| **2** | **120** | **6** |  |
| **3** | **180 (Lower deck)** | **8.5** | **7.4m (Lower deck)** |
| **4** | **180 (Lower deck)** | **5.99** | **7.55m (Lower deck)** |
| **5** | **\*75** | **7** |  |

* **Can be exceeded subject to Port Technical Director Approval**