**‘OUT OF GAUGE’ (ABNORMAL) LOADS FORM**

As part of the Ports Traffic Management Plan, to control the arrival of ‘Out of Gauge’ abnormal loads arriving for Export at Portsmouth International Port, pre-notification of arrival is now required.

**‘Out of Gauge’ abnormal loads are defined as:**

* **Heavy loads = Where the gross weight of the Tractor/trailer & loaded goods exceed 50000kg (gross) &/or any single axle weight exceeds 20000kg, (12000kg when bound for the Channel Islands).**
* **Dimensions of Tractor/trailer &/or load exceed:**
	+ **Height = 4.8m**
	+ **Width = 3m**
	+ **Length = 18.75m**

Notifications should be forwarded to the duty Traffic Supervisor via email at freight@portsmouth-port.co.uk **12-24 hours** before arrival at the Port. Please use this form to assist you in notifying the Port with the information we require. Should you arrive in excess of 12hrs prior to shipment, charges may apply.

|  |  |
| --- | --- |
| **HAULAGE COMPANY** |       |
| **CONTACT NAME** |       |
| **ADDRESS** |       |
| **TELEPHONE** |       |
| **EMAIL** |       |

|  |  |
| --- | --- |
| **FERRY COMPANY** | Choose an item. |
| **SAILING DATE** | Enter a date. | **SAILING TIME** |       |
| **FERRY DESTINATION** | Choose an item. |
| **ACCOMPANIED / UNACCOMPANIED SHIPMENT** | Choose an item. |
|  |  |
| **TRACTOR REGISTRATION** |       |
| **TRAILER REGISTRATION OR UNIT ID TO BE SHIPPED** |       |
| **DETAILS OF LOAD***(please provide length, width, height & weight)* | ***LENGTH*** | ***WIDTH*** | ***HEIGHT*** | ***WEIGHT*** |
|  |       |       |       |       |
| **Please confirm that you have received approval to ship from your respective carrier. (Yes/No)** | Choose an item. |